 LWA1 Status 

Station Status

(1s blink)

Green

All subsystems are operating normally.

Yellow

Not all subsystems are operating normally but no error condition is present.

Red

One or more subsystems are in error.

Data Operations

(One to Six ¼ s blinks)

Green

One or more data recorders are recording raw data.

Blue

One or more data recorders are recording data in spectrometer mode.

Purple

LASI is running and updating LWATV.